( TL19E1AE34150339125KBAT00 )

M/T Shift Lever Housing Replacement

1. Position the shift cables (A) on their route correctly, and align the socket holder (B) on the shift cables with the slot in the bracket base (C), then slide the holder into the base. Install the shift cable ends (D) to the shift lever assembly (E) then install the shift lever assembly.
   NOTE: When installing the shift cable (shift lever side), position the indent shape (F) to the upper side.