( TL19E1PE10410424251KCAT00 )

A/T End Cover Installation

1. For K24Z3 engine model: Set a transmission range switch (A) to the N position. Align the cutouts (B) on the rotary-frame with the neutral positioning cutouts (C) on the transmission range switch, then put a 2.0 mm (0.08 in.) feeler gauge (D) or feeler gauge blade in the cutouts to hold transmission range switch in the N position.
   NOTE: Be sure to use a 2.0 mm (0.08 in.) feeler gauge, feeler gauge blade, or equivalent to hold the transmission range switch in the N position.