( TL19E00B20200014201KBAT20 )

Front Knuckle Ball Joint Replacement

1. Raise the front of the vehicle, and support it with safety stands in the proper locations.

1. Remove the front wheel.

1. With HID lamp model: If removing the left side ball joint, disconnect the suspension stroke sensor and the lower arm.

1. Remove the wheel speed sensor harness bracket (A) and the wheel speed sensor (B) from the knuckle. Do not disconnect the wheel speed sensor connector.