( TL19E000000000K0061BAAT00 )

Service Precautions

- Use a probe with a tapered tip.

- Refer to the instructions in the Honda Terminal Kit for identification and replacement of connector terminals.

- Puncturing the insulation on a wire can cause poor or intermittent electrical connections.
- For testing at connectors, bring the tester probe into contact with the terminal from the connector side of wire harness connectors in the engine compartment.
  For female connectors, just tough lightly with the tester probe and do not insert the probe.