( TL19E00J26351559905FHAT00 )

Multi-information Display Select/Reset/Information Switch Test/Replacement

1. Measure resistance between the select/reset/information switch 7P connector No. 2 and No. 6 terminals in each switch position according to the table.

Position | Resistance
--- | ---
▲ | About 33 Ω
SEL/RESET | About 1,043 Ω
▼ | About 363 Ω

1. If the resistance is not as specified, replace the switch.

1. If the switch is OK, but there is a problem with the switch function, check the steering switches harness and cable reel.