( TL19E1PE1041074485AFAAT00 )

A/T Paddle Shifter + (Upshift Switch) Illumination Circuit Troubleshooting

1. Measure the voltage between cable reel 20P connector terminal No. 10 and body ground.

Is there battery voltage?

YES | - | Go to Step 9 .
NO | - | Check for a blown No. 6 (7.5 A) fuse in the passenger's under-dash fuse/relay box. If the fuse is OK, repair open or short in the wire between cable reel 20P connector terminal No. 10 and the passenger's under-dash fuse relay box.■

1. Turn the ignition switch to LOCK (0).

1. Disconnect the gauge control module connector.