( TL19E20A32200043502NAAT00 )

Oil pump

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Oil pump | Inner-to-outer rotor clearance |  | 0.02−0.16 mm (0.001−0.006 in.) | 0.20 mm (0.008 in.)
Pump housing-to-outer rotor clearance |  | 0.100−0.175 mm (0.0039−0.0069 in.) | 0.20 mm (0.008 in.)
Pump housing-to-outer rotor axial clearance |  | 0.02−0.07 mm (0.001−0.003 in.) | 0.12 mm (0.005 in.)
Relief valve, oil pressure with oil temperature at 80 °C (176 °F) | At idle | 70 kPa (0.7 kgf/cm 2 , 10 psi) min.
At 3,000 rpm (min −1 ) | 340 kPa (3.5 kgf/cm 2 , 50 psi) min.