( TL19E00J54226562100DCAT00 )

Under-hood Fuse/Relay Box Connector Locations

Under-hood Fuse/Relay Box

Socket | Ref | Terminal | Connects to | Notes
--- | --- | --- | --- | ---
A (Electrical load detector) | 11 | 3 | Left engine compartment wire harness |
A/C compressor clutch relay | 12 | 4 |  |
B | 14 | 14 | Left engine compartment wire harness |
Blower motor relay | 1 | 4 |  |
C | 13 | 5 | Left engine compartment wire harness |
Electronic throttle control system (ETCS) control relay | 6 | 4 |  |
Horn relay | 2 | 4 |  |
Ignition coil relay | 5 | 4 |  |
PGM-FI main relay 1 (FI MAIN) | 3 | 4 |  |
PGM-FI subrelay | 4 | 4 |  |
Radiator fan relay | 7 | 4 |  |
Rear window defogger relay | 8 | 4 |  |
T101 | 9 | ——— | Engine wire harness *1 or Starter subharness *2 |
T102 | 10 | ——— | Engine wire harness *1 or Starter subharness *2 |

*1: | R20A3 engine
*2: | K24Z3 engine