( TL19E00G10110112011FEAT00 )

A/C Compressor Clutch Check

1. Measure the clearance between the rotor pulley (A) and the armature plate (B) all the way around. If the clearance is not within specified limits, remove the armature plate and add or remove shims as needed to increase or decrease clearance.

   Clearance: | 0.35−0.65 mm (0.014−0.026 in.)

   NOTE: The shims are available in four thicknesses: 0.1 mm, 0.2 mm, 0.4 mm, and 0.5 mm.