( TL19E00J26220250671KDAT00 )

Glove Box Refrigerator Valve Removal/Installation

NOTE:

- Take care not to scratch the dashboard and its related parts.
- When removing components, use the trim tools or equivalent.

1. Open the glove box.

1. Using the appropriate trim tool, pry up on the edge of the glove box refrigerator valve (A) to release the hooks (B), then remove the valve.

1. Install the trim in the reverse order of removal, and push the hooks into place securely.