( TL19E00G10100000000MAAT00 )

A/C System Inspection

1. Check the A/C condenser for material clogging the fins or for damage to the fins:
   - Carefully clean any material from the A/C condenser fins with water and detergent.
   - Be sure to dry the A/C condenser (A) completely.

1. Inspect the drive belt, R20A3 engine model, K24Z3 engine model.

1. Make sure no material is blocking the airflow to the A/C condenser.

1. Check the dust and pollen filter, and replace it if it is clogged.

1. Start the engine, turn the air conditioning system on, and allow it to normalize for a few minutes.

1. Check that the A/C operates at each position of the blower fan switch (except OFF).