( TL19E1RE10436445401KBAT00 )

A/T Interlock System - Park Pin Switch/Shift Lock Solenoid Harness Replacement

1. Remove the harness wire ties (A), and remove the screw (B) securing the park pin switch (C), and remove the light bulb (D) from the socket.

1. Remove the A/T gear position indicator panel light harness (E), the park pin switch harness (F), and the shift lock solenoid harness (G) from the harness guide, replace the park pin switch.

1. Apply non-hardening thread lock sealant to the screw threads. Install a new park pin switch, and secure the park pin switch with the screw.

1. Tie the harnesses of the A/T gear position indicator panel light harness, the park pin switch harness, and the shift lock solenoid harness at the guide with new harness wire ties.

1. Install the A/T gear position indicator panel light bulb in the socket.