( TL19E00B20200062201KBAT00 )

Front Upper Arm Replacement

Special Tools Required
Ball joint remover, 28 mm
07MAC-SL00201

1. Raise the front of the vehicle, and support it with safety stands in the proper locations.

1. Remove the front wheel.

1. Remove the front damper/spring.

1. Remove the cotter pin (A) from the upper arm ball joint, then remove the castle nut (B).

1. Disconnect the upper arm ball joint from the knuckle using the ball joint remover.