( TL19E00K773000Y1828FAAT00 )

DTC Troubleshooting: B1828

1. Measure the voltage between power seat control unit connector A (40P) terminals No. 15 and No. 29.

Is there battery voltage when the recline switch is operated?

YES | - | Replace the recline motor/position sensor.■
NO | - | Replace the power seat control unit .■

1. Turn the ignition switch to LOCK (0).

1. Disconnect power seat control unit connector B (18P).

1. Disconnect the recline motor/position sensor 5P connector.