( TL19E00J4616185367BKBAT00 )

Front Seat Slide Motor Replacement

1. Remove the screws, then remove the slide motor (A) from the slide motor bracket (B).

1. Install the motor in the reverse order of removal, and note these items:
   - Apply multipurpose grease to the worm gear portions in both seat tracks.
   - Before installing the slide motor to the slide motor bracket, install the short flex cable to the slide motor.
   - Make sure the short flex cable and the flex cable are connected properly.