( TL19E00K761000N2601FAAT00 )

DTC Troubleshooting: 2601

DTC 2601:
Display Diag: Connect
NOTE:

- Check for B-CAN DTCs and resolve them before troubleshooting.
- Before you troubleshoot, make sure to follow the general troubleshooting information.

1. Clear the hard error code.

1. Turn the ignition switch to LOCK (0), and then back to ON (II).

1. Go into the Diagnostic Menu and select the Self-Diagnosis Mode in the Select Diagnosis Items menu.

1. Check the System Links.

Is the Display icon red?

YES | - | Go to Step 5 .
NO | - | Intermittent failure, the system is OK at this time.■

1. Check for poor connections or loose terminals at navigation unit connector B (32P), and audio unit connector E (14P).

Are there connections OK?

YES | - | Go to Step 5 .
NO | - | Repair poor connections or loose terminals, and recheck the self-diagnosis mode. ■

1. Turn the ignition switch to LOCK (0).

1. Disconnect navigation unit connector B (32P) and the navigation display unit 28P connector.

1. Connect the navigation control unit connector B (32P) terminals No. 10 and No. 26 with a jumper wire.