( TL19E1PE10410800000FEAT00 )

A/T Pressure Test

Special Tools Required
A/T oil pressure gauge set
07406-0020005
NOTE:

- Disable the VSA by pressing the VSA OFF switch.
- ABS or VSA DTC(s) may come on during the test-drive. If the ABS or VSA DTC(s) come on, clear the DTC(s) with the HDS.

1. Make sure the transmission fluid is filled to the proper level.

1. Raise the vehicle on a lift, or apply the parking brake, block the rear wheels, and raise the front of the vehicle. Make sure it is securely supported.

1. Allow the front wheels to rotate freely.

1. Remove the splash shield.

1. Connect the HDS to the DLC (A) located under the driver's side of the dashboard.

1. Turn the ignition switch to ON (II). Make sure the HDS communicates with the PCM. If it does not, go to the DLC circuit troubleshooting; R20A3 engine model, K24Z3 engine model.