( TL19E00K791000R922XFAAT00 )

DTC Troubleshooting: 92-2x

1. Measure the resistance between No. 20 terminal of SRS unit connector A (39P) and body ground. There should be more than 1 MΩ.

Is the resistance as specified?

YES | - | Faulty SRS unit or passenger's airbag off indicator; replace the passenger's airbag off indicator. If the problem is still present, replace the SRS unit. ■
NO | - | Short to ground in the dashboard wire harness or the audio wire harness; replace the faulty harness.■