( TL19E20A14400065081KDAT00 )

Water Outlet Removal and Installation

Installation

1. Remove all of the old liquid gasket from the water outlet mating surfaces, bolts, and bolt holes.

1. Clean and dry the water outlet mating surfaces.

1. Apply liquid gasket (P/N 08C70-K0234M, 08C70-K0334M, or 08C70-X0331S) to the cylinder head mating surface of the water outlet.
   NOTE:
   - Apply liquid gasket about 2.5 mm (0.098 in.)diameter bead along the broken line (A).
   - Do not install components if 5 minutes or more have passed after applying the liquid gasket. Instead, remove the old residue and reapply the liquid gasket.