( TL19E00K80100081310FAAT00 )

DTC Troubleshooting: 31, 32, 33, 34, 35, 36, 37, 38

DTC 31, 32, 33, 34, 35, 36, 37, 38:
ABS Solenoid

1. Turn the ignition switch to ON (II).

1. Clear the DTC with the HDS.

1. Turn the ignition switch to LOCK (0), then turn it to ON (II) again.

1. Check for DTCs with the HDS.

Is DTC 31, 32, 33, 34, 35, 36, 37, or 38 indicated?

YES | - | Go to Step 5 .
NO | - | The system is OK at this time.■

1. Update the VSA modulator-control unit if it does not have the latest software. If the unit already has the latest software, substitute a known-good VSA modulator-control unit.

1. Turn the ignition switch to LOCK (0), then turn it to ON (II) again.

1. Check for DTCs with the HDS.

Is DTC 31, 32, 33, 34, 35, 36, 37, or 38 indicated?

YES | - | Check for loose terminals in the VSA modulator-control unit 47P connector. If the VSA modulator-control unit was updated, substitute a known-good VSA modulator-control unit, then retest. If the VSA modulator-control unit was substituted, go to Step 1 .
NO | - | If the VSA modulator-control unit was updated, troubleshooting is complete. If the VSA modulator-control unit was substituted, replace the original VSA modulator-control unit. If any other DTCs are indicated, go to the indicated DTCs troubleshooting.■