( TL19E1PE10410917451KAAT00 )

A/T Countershaft Reverse Selector Hub and 3rd Gear Removal

Special Tools Required
Bearing separator
07KAF-PS30200

1. Install the bearing separator on 4th gear (A). Set a press on the countershaft (B) with a spacer (C) between the press and the countershaft, and remove the reverse selector hub (D).
   NOTE: Some reverse selector hubs are not press-fitted, and can be removed without using the bearing separator and a press.

1. Remove the needle bearing, the set ring, the 35 x 47 x 7.8 mm collar, and the 31 mm cotters.

1. Set the press on the countershaft (A) with a spacer (B) between the press and the countershaft, and remove 3rd gear (C).

1. Remove the 37 x 41 x 54.3 mm collar, 5th gear, 1st gear, and 2nd gear.