( TL19E00H46400000000AAAT00 )

SRS Precautions and Procedures

Seats with Side Airbags
Seats with side airbags have a ‘‘SIDE AIRBAG'' label on the seat-back.

- When cleaning, use a damp cloth to clean the seat. Do not soak the seat with liquid. Do not spray steam on the seat.
- Do not repair a torn or frayed seat-back cover. Replace the seat-back cover.
- After a collision where the side airbag was deployed, replace the side airbag and seat frame with new parts. If the seat-back cushion is split, it must be replaced.
- Never put aftermarket accessories on the seat (covers, pads, seat heaters, lights, etc.).