( TL19E00K791000R7422FAAT00 )

DTC Troubleshooting: 74-22

1. Check resistance between the No. 1 and No. 2 terminals of right side E-pretensioner motor 2P connector. There should be 0−1.0 Ω.

Is the resistance as specified?

YES | - | Open in the left engine compartment subharness (LHD models), the E-pretensioner subharness (RHD models), left engine compartment wire harness, right side wire harness or right engine compartment wire harness; replace the faulty harness.■
NO | - | Faulty the right side E-pretensioner motor; replace the right side E-pretensioner motor. ■