( TL19E1PE10411239521KBAT00 )

Torque Converter Housing Mainshaft Bearing and Oil Seal Replacement

Special Tools Required
Adjustable bearing remover set
07JAC-PH80000
Driver handle 15 x 135L
07749-0010000
Bearing driver attachment 62 x 68 mm
07746-0010500
Bearing driver attachment 72 x 75 mm
07746-0010600

1. Remove the mainshaft bearing and the oil seal using the adjustable bearing remover set.

1. Install a new mainshaft bearing until it bottoms in the torque converter housing using the 15 x 135L driver handle and the 62 x 68 mm bearing driver attachment.

1. Install a new oil seal flush with the torque converter housing using the 15 x 135L driver handle and the 72 x 75 mm bearing driver attachment.
   NOTE: Do not drive the seal into the torque converter housing until it bottoms out; it will block the fluid return passage and cause transmission damage.