( TL19E20A14600017811KAAT00 )

Cylinder Head Cover Removal

1. Do the battery terminal disconnection procedure.

1. Remove the harness cover.

1. Remove the injector cover.

1. Disconnect the four ignition coil connectors. Remove the four bolts (A) securing the harness holders, then remove the front harness holder (B) from the bracket.

1. Disconnect the alternator connector (A) and the BLK wire (B) from the alternator.

1. Disconnect the A/C compressor clutch connector (C), and remove the harness clamp (D).

1. Remove the dipstick (A) and the breather hose (B).

1. Remove the cylinder head cover.