( TL19E20A14616700000MAAT00 )

Camshaft Inspection

1. Check the total runout with the camshaft supported on V-blocks.
   - If the total runout of the camshaft is within the service limit, replace the cylinder head.
   - If the total runout is beyond the service limit, replace the camshaft, and recheck the oil clearance. If the oil clearance is still out of tolerance, replace the cylinder head.
   Camshaft Total Runout

   Standard (New): | 0.03 mm (0.001 in.) max.
   Service Limit: | 0.04 mm (0.002 in.)