( TL19E1PE10411239511KCAT00 )

A/T Housing Bearing Installation

Special Tools Required
Bearing driver attachment 78 x 80 mm
07NAD-PX40100
Driver handle 15 x 135L
07749-0010000
Bearing driver attachment 42 x 47 mm
07746-0010300
Snap ring pliers
07LGC-0010100

1. Install the bearings in the direction shown.

1. Expand each snap ring using snap ring pliers, and install the mainshaft bearing (A) and the countershaft bearing (B) part-way into the transmission housing using the 15 x 135L driver handle and the 78 x 80 mm bearing driver attachment.

1. Release snap ring pliers, then push the bearing down into the transmission housing until the snap ring snaps in place around it.