( TL19E00000000000000JBAT40 )

Maintenance Schedule for Normal and Severe Conditions - except EU, Australia, New Zealand, and South Africa

This maintenance schedule outlines the minimum required maintenance that you should perform to ensure the trouble-free operation of the vehicle. Due to regional and climatic differences, some additional service may be required. Please consult the warranty booklet for a more detailed description.
The following items must be used for ‘‘severe conditions'' indicated on schedule, if the vehicle is driven MAINLY under the specified conditions A to E.

- Engine oil and engine oil filter: A/B/C/D/E
- Transmission fluid: B/D

A: Driving less than 8 km (5 miles) per trip or, in freezing temperatures, driving less than 16 km (10 miles) per trip.
B: Driving in extremely hot over 35 °C (95 °F) conditions.
C: Extensive idling, or long periods of stop-and-go driving.
D: Towing trailer, driving with a loaded roof rack, or driving in mountainous conditions.
E: Driving on muddy, dusty, or de-iced roads.

Service at the indicated distance or time whichever comes first | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12.5 | 25.0 | 37.5 | 50.0 | 62.5 | 75.0 | 87.5 | 100.0 | 112.5 | 125.0
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Replace engine oil R20A3, K24Z3 | Normal Conditions | Every 10,000 km (6,250 miles) or 1 year
Severe Conditions | Every 5,000 km (3,125 miles) or 6 months
Replace engine oil filter R20A3, K24Z3 | Normal Conditions | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
Severe Conditions | Every 10,000 km (6,250 miles) or 6 moths
Replace air cleaner element R20A3, K24Z3 | Every 30,000 km (18,600 miles)
Inspect valve clearance R20A3, K24Z3 | Every 40,000 km (25,000 miles)
Replace fuel filter R20A3, K24Z3 Replace fuel filter every 40,000 km (25,000 miles) or 2 years, if the fuel the customer uses is suspected to be contaminated. |  |  |  | ● |  |  |  | ● |  |
Replace spark plugs R20A3, K24Z3 | Every 100,000 km (62,500 miles)
Inspect drive belt R20A3, K24Z3 Look for cracks and damage, then check the position of the drive belt auto-tensioner indicator. |  | ● |  | ● |  | ● |  | ● |  | ●
Inspect idle speed R20A3, K24Z3 |  |  |  |  |  | ● |  |  |  |
Replace engine coolant R20A3, K24Z3 Use genuine Honda All Season Antifreeze/Coolant Type 2. | At 200,000 km (120,000 miles) or 10 years, then every 100,000 km (60,000 miles) or 5 years
Replace Manual Transmission Fluid. Use genuine Honda MTF. | Normal Conditions |  |  |  |  |  | ● |  |  |  |
Severe Conditions |  |  | ● |  |  | ● |  |  | ● |
Replace Automatic Transmission Fluid. Use genuine Honda ATF-Z1. | Normal Conditions |  |  |  |  |  | ● |  |  |  | ●
Severe Conditions |  |  | ● |  | ● |  | ● |  | ● |

| Only severe schedule is required in some countries, refer to local warranty booklet.

Service at the indicated distance or time whichever comes first | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12.5 | 25.0 | 37.5 | 50.0 | 62.5 | 75.0 | 87.5 | 100.0 | 112.5 | 125.0
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120

Check front and rear brakes

- Check the brake pad and disc thickness. Check for damage or cracks.
- Check the calipers for damage, leaks, and tightness.

●

●

●

●

●

●

●

●

●

●

Replace brake fluid

- Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid.
- Check the brake fluid level is between upper and lower marks on the reservoir.

Every 3 years

Check parking brake adjustment Check the parking brake operation. | ● | ● |  | ● |  | ● |  | ● |  | ●
Replace dust and pollen filter (if equipped) | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
Check expiration date for TRK (Temporary Repair Kit) bottle (if equipped)
Rotate tyres Check tyre inflation and condition at least once per month. | Every 10,000 km (6,250 miles)

Visually inspect the following items:

- Check for correct installation and position, check for cracks, deterioration, rust, and leaks.
- Check tightness of screws, nuts, and joints. If necessary, retighten.

Tie-rod ends, steering gearbox, and boots

- Check rack grease and steering linkage.
- Check the boot for damage and leaking grease.

Every 10,000 km (6,250 miles) or 6 months

Suspension components

- Check the bolts for tightness.
- Check all dust covers for deterioration and damage.

Driveshaft boots

- Check the boot and boot band for cracks.
- Check rack grease.

Brake hoses and lines (including VSA lines) Check the master cylinder and VSA modulator-control unit and leakage. | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●

All fluid levels and condition of fluids
Check levels and check for leaks. If necessary, add.

- Engine coolantR20A3, K24Z3
- MTF
- ATF
- Brake fluid
- Clutch fluid
- Windshield washer fluid

Exhaust system R20A3, K24Z3 Check the exhaust pipe and muffler for damage, leaks, and tightness.

Fuel line R20A3, K24Z3
and connections R20A3, K24Z3

- Check fuel lines for loose connections, cracks, and deterioration.
- Retighten loose connections and replace any damaged parts.