( TL19E00B20200014201KBAT20 )

Front Knuckle Ball Joint Replacement

Special Tools Required
C-frame
070AF-S5A0310
Air hammer attachment
070AF-TA00310
Attachment, 53 x 50 mm
070AF-TA00320
Ball joint base attachment, 62 x 50 mm DP77
070AF-TA00330
Ball joint remover, 28 mm
07MAC-SL00201
NOTE:

- When use the air hammer, confirms that the tank of the air compressor filled with air and gauge of the tank shows more than 440 kPa (4.5 kgf/cm 2 , 64 psi).
- Replace the knuckle as an assembly if the knuckle ball joint has the paint mark (A). Paint mark indicate the ball joint has been replaced.