( TL19E00B20200037701KDAT00 )

Front Lower Arm Removal/Installation

Compliance Bushing Replacement

1. Remove the lower arm.

1. Mark alignment marks (A) on the bottom of the lower arm next to the aligning marks (B) on the compliance bushing.
   NOTE: The compliance bushing has a specific installation position. Turn the lower arm so that its bottom side is up. Position the bushing identifying mark (C) face up and near the tab (D) on the lower arm. Then align the bushing aligning marks on the bushing and the lower arm.
   If the alignment marks are gone, align the angle (E) between the lower arm and the bushing as shown.

Aligning the marking position
Aligning the angle (reference)