( TL19E00G10110249112FAAT00 )

Radiator and A/C Condenser Fan Low Speed Circuit Troubleshooting

1. Measure the voltage between the A/C condenser fan 2P connector No. 1 and No. 2 terminals.

Is there battery voltage?

YES | - | Replace the A/C condenser fan motor. ■
NO | - | Check for an open in the wire between the A/C condenser fan and body ground. If the wire is OK, check for poor ground at G301, LHD model, RHD model. ■

1. Turn the ignition switch to LOCK (0).

1. Remove the relay circuit board.