( TL19E00K75100081110FAAT00 )

DTC Troubleshooting: 11, 17

1. Check for continuity between LKAS control unit 26P connector No. 25 terminal and PCM connector A (49P) No. 4 terminal.

Is there continuity?

YES | - | Check for loose terminals in the PCM connector A, and LKAS control unit connector, and repair if necessary. If all connections are OK, replace the PCM. ■
NO | - | Repair an open in the wire between the LKAS control unit and the branch of the F-CAN line (CANL).■