( TL19E00D14300014791MDAT10 )

Front Brake Pad Inspection and Replacement

1. Pivot the caliper down into position. Install the flange bolt (A), and tighten it to the specified torque.

1. Install the brake hose mounting bolt (B).

1. Clean the mating surfaces of the brake disc and the inside of the wheel, then install the front wheels.

1. Press the brake pedal several times to make sure the brakes work.
   NOTE: Engagement may require a greater pedal stroke immediately after the brake pads have been replaced as a set. Several applications of the brake pedal will restore the normal pedal stroke.

1. Add brake fluid as needed.

1. After installation, check for leaks at hose and line joints or connections, and retighten if necessary.
   Test-drive the vehicle, then check for leaks.