( TL19E30A20326934595KBAT00 )

Injector Replacement

1. Relieve the fuel pressure.

1. Remove the engine cover.

1. Remove the quick-connect fitting cover (A), then disconnect the quick-connect fitting (B).

1. Disconnect the injector connectors (C) and the engine mount control solenoid valve connector (D).

1. Remove the ground cable bolts (G101 and G102) (E).

1. Remove the fuel rail mounting nuts (F) from the fuel rail (G).

1. Remove the fuel rail and the injectors from the injector base.

1. Remove the injector clips (H) from the fuel rail.

1. Remove the injectors from the fuel rail.

1. Relieve the fuel pressure.

1. Remove the engine cover.

1. Remove the quick-connect fitting cover (A), then disconnect the quick-connect fitting (B).

1. Disconnect the injector connectors (C) and the engine mount control solenoid valve connector (D).

1. Remove the ground cable bolts (G101 and G102) (E).

1. Remove the fuel rail mounting nuts (F) from the fuel rail (G).

1. Remove the fuel rail and the injectors from the injector base.

1. Remove the injector clips (H) from the fuel rail.

1. Remove the injectors from the fuel rail.

1. Coat the new O-rings (black) (A) with clean engine oil, and insert the injectors (B) into the fuel rail (C).

1. Install the injectors clips (D).

1. Coat the new injector O-rings (brown) (E) with clean engine oil.

1. Install the fuel rail and the injectors in the injector base (F).

1. Install the fuel rail mounting nuts (G) and the ground cable bolts (G101 and G102) (H).

1. Connect the injector connectors (I) and the engine mount control solenoid valve connector (J).

1. Connect the quick-connect fitting (K), and quick-connect fitting cover (L).

1. Turn the ignition switch to ON (II), but do not operate the starter. After the fuel pump runs for about 2 seconds, the fuel rail will be pressurized. Repeat this two or three times, then check for fuel leakage.

1. Reinstall the engine cover.

1. Coat the new O-rings (black) (A) with clean engine oil, and insert the injectors (B) into the fuel rail (C).

1. Install the injectors clips (D).

1. Coat the new injector O-rings (brown) (E) with clean engine oil.

1. Install the fuel rail and the injectors in the injector base (F).

1. Install the fuel rail mounting nuts (G) and the ground cable bolts (G101 and G102) (H).

1. Connect the injector connectors (I) and the engine mount control solenoid valve connector (J).

1. Connect the quick-connect fitting (K), and quick-connect fitting cover (L).

1. Turn the ignition switch to ON (II), but do not operate the starter. After the fuel pump runs for about 2 seconds, the fuel rail will be pressurized. Repeat this two or three times, then check for fuel leakage.

1. Reinstall the engine cover.