( TL19E00H46400016251KBAT00 )

Cable Reel Replacement

Removal

1. Make sure the front wheels are aligned straight ahead.

1. Do the battery terminal disconnection procedure, then wait for 3 minutes.

1. Remove the driver's airbag.

1. Disconnect the connector (A) from the cable reel, then remove the steering wheel bolt (B).

1. Confirm that the front wheels point straight ahead, then remove the steering wheel with a steering wheel puller. Do not tap on the steering wheel or steering column shaft when removing the steering wheel.

1. Remove the column cover.