( TL19E00K791000R7661FAAT00 )

DTC Troubleshooting: 76-61, 76-62

1. Check the voltage between the No. 12 terminal of the left engine compartment subharness 14P connector (LHD models) or E-pretensioner subharness 14P connector (RHD models) and body ground. There should be battery voltage.

Is there battery voltage?

YES | - | Go to Step 10 .
NO | - | Open between the No. 20 (30 A) fuse in the front passenger's under-dash fuse/relay box and the No. 12 terminal of the left engine compartment subharness 14P connector (LHD models) E-pretensioner subharness 14P connector (RHD models).■

1. Disconnect the left engine compartment subharness 5P connector (LHD models) E-pretensioner subharness 5P connector (RHD models) from the E-pretensioner unit.