( TL19E00J36100000000MBAT00 )

Navigation System Forced Starting of Display

Special tools required
SCS Service Connector
07PAZ-0010100

1. Turn the ignition switch to LOCK (0).

1. Connect the SCS service connector (A) to the navigation service connector (B) located behind the navigation unit.

1. Turn the ignition switch to ON (II).

1. Check that the diagnosis menu for the picture diagnosis starts up, and then changes to the system link menu.
   NOTE: If the display fails to display the system link screen, refer to no picture is displayed.