( TL19E20A14680263001KBAT00 )

Cylinder Head Valve Guide Replacement

Special Tools Required
Valve guide driver, 5.35 x 9.7
07742-0010100
Valve guide reamer, 5.525 mm
07HAH-PJ70100

1. Inspect the valve stem-to-guide clearance.

1. As illustrated, use a commercially available air-impact valve guide driver (A) modified to fit the diameter of the valve guides. In most cases, the same procedure can be done using the valve guide driver and a conventional hammer.

1. Select the proper replacement guides, and chill them in the freezer section of a refrigerator for about an hour.