( TL19E00H46200053401KBAT00 )

Front Seat Belt Replacement

1. Install the seat belt and the retractor in the reverse order of removal, and note these items:
   - Apply medium strength liquid thread lock to the anchor bolts before reinstallation.
   - Tighten the bolts by hand first, then tighten to the specified torque.
   - Check that the retractor locking mechanism functions.
   - Assemble the washer, the collars, and the bushing on the upper anchor bolt, the lower anchor bolt, and the retractor bolt as shown.
   - Before installing the anchor bolts, make sure there are no twists or kinks in the seat belt.
   - Make sure the seat belt tensioner connector and the seat belt motor connector (for some models) are plugged in properly.
   - Do the battery terminal reconnection procedure.
   - Check for any DTCs that may have been set during repairs, and clear them.

Upper anchor bolt installation
Lower anchor bolt installation - driver's side
Retractor bolt installation