( TL19E30A14674317531KDAT00 )

Crankshaft Pulley Removal and Installation

Special Tools Required
Handle, 6-25-660L
07JAB-001020B
Crankshaft pulley holder, 50 offset 65
070AB-RJA0100
Socket wrench, 19 x 90L
07JAA-001020A
Removal

1. Remove the front wheels.

1. Remove the splash shield.

1. Remove the drive belt.

1. Hold the pulley with the handle (A) and the crankshaft pulley holder (B).

1. Remove the bolt with a 19 x 90L socket (C) and a breaker bar, then remove the crankshaft pulley.

Installation

1. Clean the crankshaft pulley (A), the crankshaft (B), the bolt (C), and the washer (D). Lubricate as shown.

1. Install the crankshaft pulley, and hold the pulley with the handle (A) and the crankshaft pulley holder (B).

1. Tighten the bolt to 49 N·m (5.0 kgf·m, 36 lbf·ft) with a torque wrench and a 19 x 90L socket (C). Do not use an impact wrench. If the pulley bolt or crankshaft are new, tighten the bolt to 177 N·m (18.0 kgf·m, 130 lbf·ft), then remove the bolt and tighten it to 49 N·m (5.0 kgf·m, 36 lbf·ft).

1. Tighten the pulley bolt an additional 90 °.

1. Install the drive belt.

1. Install the splash shield.

1. Install the front wheels.