( TL19E00J10300027201FHAT00 )

Speaker Test/Replacement

Rear Door Speaker (With Premium Audio System)

1. Remove the door panel.

1. Remove the bolt. Then lift the speaker straight up to release the lower clips (A).
   If you pull the speaker out too far from the door, you will damage the lower clips.

1. Disconnect the 2P connector (B), and remove the speaker.

1. Measure the resistance between the terminals No. 1 and No. 2. There should be about 4 Ω.

1. If the resistance is not as specified, replace the door speaker.