( TL19E00J10300013151BBAT00 )

Audio System Self-diagnostic Function

Speaker Check Mode
NOTE:

- Not all self-diagnostic functions appear on all models.
- There may be other self-diagnostic functions that are for factory use only.

1. Turn the ignition switch to ON (II). Turn the audio unit off.

1. Push and hold the No. 1 and No. 3 buttons. While holding the buttons, push the VOL knob to on. Release the buttons and the speaker check mode begins. A test tone should sound from one speaker.
   NOTE: Make sure the volume is set to a normal or slightly higher than normal volume and set the balance and fader to the center position.

1. Each time you press the SKIP button, the test moves to the next the speaker in the order listed.

Display Specifications

With Premium Audio System
( ) is pressed: | (1)→(2)→(3)→(4)→(5)→(6)→(7)→(8)→(9)
( ) is pressed: | (1)→(6)→(6)→(6)→(6)→(5)→(4)→(3)→(2)
( ) is pressed: | (1)→(2)→(3)→(4)→(5)
( ) is pressed: | (1)→(5)→(4)→(3)→(2)

With Premium Audio System

| Speaker | Displayed Segments | Remarks
--- | --- | --- | ---
(1) | Left front door speaker and tweeter | SPK FR-L | You should hear a low frequency tone
(2) | Front center speaker | SPK CNTR | You should hear a low frequency tone
(3) | Right front door speaker and tweeter | SPK FR-R | You should hear a low frequency tone
(4) | Right rear door speaker | SPK ST-R | You should hear a low frequency tone
(5) | Right rear speaker | SPK RR-R | You should hear a low frequency tone
(6) | Subwoofer | SPK SUBW | You should hear a low frequency tone
(7) | Left rear speaker | SPK RR-L | You should hear a low frequency tone
(8) | Left rear door speaker | SPK ST-L | You should hear a low frequency tone

(9)

All speakers

SPK ALL

- You should hear a low frequency tone
- The subwoofer does not sound a tone

Without Premium Audio System

| Speaker | Displayed Segments | Remarks
--- | --- | --- | ---
(1) | Left front door speaker and tweeter | SPK FR-L | You should hear a low frequency tone
(2) | Right front door speaker and tweeter | SPK FR-R | You should hear a low frequency tone
(3) | Right rear speaker | SPK RR-R | You should hear a low frequency tone
(4) | Left rear speaker | SPK RR-L | You should hear a low frequency tone

(5)

All speakers

SPK ALL

- You should hear a low frequency tone
- The subwoofer does not sound a tone

NOTE: Any other diagnostic screens are shown for factory use only.

1. The speaker check mode ends when you turn the audio unit off or turn the ignition switch to LOCK (0).