( TL19E00K791000R681XFAAT00 )

DTC Troubleshooting: 68-1x

1. Check for continuity between the No. 4 terminal of the dashboard wire harness 4P connector and body ground.

Is there continuity?

YES | - | Faulty SRS unit or poor connection at SRS unit connector A (39P) and the SRS unit. Check the connection between the connector and the SRS unit. If the connection is OK, replace the SRS unit. ■
NO | - | Open between the dashboard wire harness 4P connector and body ground (G504) or poor connection at G504.■