( TL19E20A18313200000LAAT00 )

Balancer Shaft/Balancer Shaft Holder Assembly Overhaul

Balancer Shaft Inspection

1. Seat the balancer shaft by pushing it away from the balancer shaft sprocket end of the balancer shaft holder.

1. Zero the dial indicator against the end of the balancer shaft, then push the balancer shaft back and forth and read the end play.

   Balancer Shaft End Play
   Front Balancer Shaft:
   Standard (New): | 0.05−0.10 mm (0.002−0.004 in.)
   Service Limit: | 0.135 mm (0.0053 in.)
   Rear Balancer Shaft:
   Standard (New): | 0.05−0.10 mm (0.002−0.004 in.)
   Service Limit: | 0.135 mm (0.0053 in.)