( TL19E00K791000REX11FAAT00 )

DTC Troubleshooting: Ex-11

DTC Ex-11 (''x'' can be 0 thru 9 or A thru F):
Control Operation Recorded
NOTE:

- Before doing this troubleshooting procedure, review SRS Precautions and Procedures and General Troubleshooting Information.
- Before replacing the SRS unit, check the SRS unit software version with the HDS. If the software version is not the latest, update the SRS unit software and retest.

1. Clear the DTC memory.

1. Turn the ignition switch to ON (II), then wait for 10 seconds.

1. Read the DTC.

Are DTC Ex-11 and Fx-11 indicated?

YES | - | The SRS unit must be replaced after any airbags and/or tensioners have deployed. ■
NO | - | Go to Step 4 .

1. Clear the DTC memory.

1. Turn the ignition switch to ON (II), then wait for 10 seconds.

1. Read the DTC.

Is DTC Ex-11 indicated?

YES | - | Faulty SRS unit; replace the SRS unit. ■
NO | - | Intermittent failure, the system is OK at this time. Go to Troubleshooting Intermittent Failures. If another DTC is indicated, troubleshoot the DTC.