( TL19E00R11100000000YCAT09 )

Roof and Side Panel Construction

NOTE: Confirm that the sold as repair parts, refer to the appropriate Parts Catalog.
NOTE:

- The part marked with numbers are sold as repair parts.
- The part marked with letters are not sold separately and are shown only for reference.
- [ ]: Thickness unit: mm (in.)
- High-tension steel sheet: Tensioner strength 340 to 590 MPa.

No. | Part Name | Tensioner Strength (MPa) | Zinc-plating
--- | --- | --- | ---
(1) | Roof Panel [0.65 (0.026)] | 270 |
(2) | Front Roof Rail [0.6 (0.024)] | 270 |
(3) | Rear Roof Rail Upper [0.6 (0.024)], Lower [1.2 (0.047)] | 270 |
(4) | Roof Arch A [0.8 (0.031)] | 590 |
(5) | Side Sill Outer Panel [0.7 (0.028)] | 270 | ○
(6) | Front Side Outer Panel Set [0.7 (0.028)] | 270 | ○
(7) | Rear Side Outer Panel Set [0.7 (0.028)] | 270 | ○
(8) | Front Pillar Stiffener Comp.
| a: | Front Pillar Upper Stiffener [1.2 (0.047)] | 590 |
b: | Roof Side Stiffener [1.2 (0.047)] | 590 |
(9) | Center Pillar Stiffener Comp.
| a: | Center Pillar Lower Stiffener [0.9 (0.035)] | 590 |
b: | Center Pillar Upper Stiffener [1.8 (0.071)] | 590 |
(10) | Side Sill Reinforcement Comp.
| a: | Front Pillar Lower Stiffener [0.8 (0.031)] | 590 | ○
b: | Side Sill Reinforcement [1.6 (0.063)] | 590 | ○
(11) | Rear Gutter Comp.
| a: | Rear Gutter Upper, Lower [0.7 (0.028)] | 270 | ○
b: | Rear Combination Adapter [0.6 (0.024)] | 270 | ○
(12) | Front Inner Upper Pillar Set
| a: | Front Inner Upper Pillar [2.3 (0.091)] | 590 |
b: | Front Pillar Inner Upper Extension[1.4 (0.055)] | 440 |
(13) | Front Inner Lower Pillar Set
| a: | Front Inner Lower Pillar [1.2 (0.047)] | 590 | ○
b: | Front Jack-Up Bracket [2.0 (0.079)] | 590 | ○
(14) | Roof Side Rail [2.0 (0.079)] | 590 |
(15) | Center Inner Pillar [1.4 (0.055)] | 440 |
(16) | Rear Inner Panel Comp.
-1 | Rear Inner Panel | 270 | ○
-2 | Rear Wheel Arch Extension Comp. |  |
a: | Rear Wheel Arch Extension [0.6 (0.024)] | 270 | ○
b: | Side Sill Reinforcement Rear Extension [1.6 (0.063)] | 440 | ○
c: | Rear Jack-Up Bracket [2.0 (0.079)] | 590 | ○
-3 | Rear Wheelhouse [0.8 (0.031)]/Damper Base [2.3 (0.091)] | 270 | ○
(17) | Front Door | Skin [0.8 (0.031)] | 340 | ○
Panel Front [1.4 (0.055)], Rear [0.7 (0.028)] | 270 | ○
(18) | Rear Door | Skin [0.8 (0.031)] | 340 | ○
Panel Front [1.2 (0.047)], Rear [0.65 (0.026)] | 270 | ○