( TL19E00K791000R8561FAAT00 )

DTC Troubleshooting: 85-61, 85-62

DTC 85-61:
No Signal From the OPDS Unit
DTC 85-62:
Non Stipulated Data From the OPDS Unit
NOTE: Before doing this troubleshooting procedure, review SRS Precautions and Procedures and General Troubleshooting Information.

1. Clear the DTC memory.

1. Read the DTC.

Is DTC 85-61 or 85-62 indicated?

YES | - | Go to Step 3 .
NO | - | Intermittent failure, the system is OK at this time. Go to Troubleshooting Intermittent Failures. If another DTC is indicated, troubleshoot the DTC.

1. Check the No. 12 (7.5 A) fuse in the driver's under-dash fuse/relay box.

Is the fuse OK?

YES | - | Go to Step 4 .
NO | - | Replace the fuse, then turn the ignition switch to ON (II). If the fuse blows again, check for a short in the No. 12 (7.5 A) fuse circuit (dashboard wire harness, right side wire harness, SRS floor wire harness, or OPDS unit harness).

1. Disconnect the OPDS unit harness 18P connector (A) from the OPDS unit.

1. Turn the ignition switch to ON (II).