( TL19E00E16226600000LDAT00 )

Driveshaft Reassembly

1. Adjust the length (A) of the driveshafts to the figure as shown, then adjust the boots to halfway between full compression and full extension. Bleed excess air from the boots by inserting a flat-tipped screwdriver between the boot and the joint.

Model | Left/Right Driveshaft | Specified Length (A)
--- | --- | ---
R20A3 engine model | M/T | Left | 559−564 mm (22.01−22.20 in.)
Right | 547−552 mm (21.54−21.73 in.)
A/T | Left | 557−562 mm (21.93−22.13 in.)
Right | 545−550 m (21.46−21.65 in.)
K24Z3 engine model | M/T | Left | 559−564 mm (22.01−22.20 in.)
Right | 481−486 mm (18.94−19.13 in.)
A/T | Left | 554−559 mm (21.81−22.01 in.)
Right | 480−485 mm (18.90−19.09 in.)

1. Install new boot bands.
   - For the double loop type, go to Step 11 .
   - For the low profile type, go to Step 20 .

Left driveshaft
Right driveshaft