( TL19E1AE34116317010KBAT00 )

Clutch Hose Replacement

NOTE:

- Replace the clutch hose if the hose is twisted, cracked, or if it leaks.
- Use fender covers to avoid damaging painted surfaces.
- Do not spill brake fluid on the vehicle; it may damage the paint or plastic. If brake fluid does contact the paint or plastic, wash it off immediately water.

1. Do the battery removal procedure.

1. Disconnect the ECM connectors, then remove the ECM: R20A3 engine model, K24Z3 engine model.

1. Remove the ground cable clamp (A), upper battery base mounting bolts (B), and loosen the under battery base mounting bolts (C), then remove the battery base (D).