( TL19E00J18573560321KBAT00 )

Trunk Lid Cylinder Replacement

1. Remove the bolt, and release the hook (A) by turning the trunk lid cylinder (B) 45 °, then remove the cylinder from the key cylinder bracket (C).

1. Install the cylinder reverse order of removal, and note these items:
   - Replace the damaged cable fastener with a new one.
   - Make sure the opener cable is connected properly.
   - When installing the bracket, first tighten the inside mounting bolt, then tighten the outside mounting bolt.
   - Make sure the trunk lid opens properly and locks securely.